{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["predmer"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"predmer","index":0,"n_rows":61,"n_cols":6,"rows_kept":61,"merged":[[3,1,3,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[33,1,33,2],[48,1,48,2],[52,0,52,5]],"flags":["formulas_cached_only"]}
[]
[null,null,"PREDMER I PREDRAČUN"]
[]
["I","INSTALACIJA RAČUNARSKE INSTALACIJE"]
[]
[null,"tip","opis","kol","cena","ukupno"]
[1,"REK orman 22HU   1080x600x600mm,","(22HU/19\" rek orman stojeći, staklena vrata sa bravom, točkići i nožice sa nivelacijom, prednje i zadnje šine 19\" sa brojevima unita, dim. 1080x600x600mm), referenca DS226060-A",1]
[2,"krovni ventilatorski panel ","(19\" krovni ventilator panel sa 2 ventilatora i termostatom za stojeće rek ormane), referenca DLT 44802-A",1]
[3,"Polica za rek dubine 450mm","(Polica fiksna - za sve tipove rek ormana dubine 450mm , 1HU, 80kg max, perforirana) referenca DFS14845-C",3]
[4,"Napojni panel sa 7 utičnih mesta","19\" napojni panel 7xšuko i prekidač, PVC, 1.25HU referenca IU070107-B",1]
[5,"RJ 45 modul","(TOOLLESS LINE RJ-45 modul UTP cat 6), referenca HSERMRJGWS",30]
[6,"Patch panel sa 24 RJ-45 UTP cat6","(TOOLLESS LINE Patch panel 19\"/1HU sa 24 RJ-45 UTP cat 6, prazan), referenca HSER0240GS",4]
[7,"Voice panel sa 24 RJ-45 UTP cat6","(telefonski patch panel 19\" cat.3, 25xRJ45, UTP, 4 pina, referenca HSERU25IGC",1]
[8,"slepa maska za panel","(TOOLLESS LINE -slepa maska za panele i utičnice referenca HSERMRZ01WF",66]
[9,"ranžer kablova","(19\" panel za ranžer kablova, 5 većih PVC prstenova 80x40mm, 1HU), referenca DBK1485",2]
[10,"ranžirni prsten","ranžirni prsten 40x80mm za vertikalno ranžiranje referenca DBKO4080",8]
[11,"panel sa četkom","panel sa četkom za krovni ulaz kablova, za DS/DSZ/DSS, 2HU, referenca DBK24800",1]
[12,"polucilindar","polucilindar EK333 sa jednim ključem, referenca DV900333",1]
[13,"set za fiksiranje opreme","(19\" set za fiksiranje opreme M6 (vijak+kavez matica,50komada), referenca DSSRA050",1]
[14,"Priključnica RJ-45 UTP cat6 Mozaik Legrand ili sličan","(Priključnica RJ-45 UTP  cat6). Referenca 076561 Montiraju se u iste montažne kutije ili podne kutije sa energetskim priključnicama.",30]
[15,"Kabal UTP cat6 ","(kabal instalacioni cat6 UTP - ",1200]
[16,"Gibljiva cev instalaciona 16mm ","(gibljiva instalaciona cev halogen free) (m) isporuka i montaža ",700]
[17,"Cev instalaciona 23mm HF","(cevi instalacione halogen free) (m) isporuka i montaža ",150]
[18,"HDMI kabal dužine 10m","nabavka i isporuka HDMI kabla dužine 10m, za montažu između projektora i kompjutera u kabinetima.",2]
[19,"HDMI kabal dužine 25m","nabavka i isporuka HDMI kabla dužine 10m, za montažu između projektora i kompjutera u kabinetima.",1]
[20,"Priključnica HDMI Mozaik Legrand ili sličan","(Priključnica HDMI). Referenca 078778 Montiraju se u iste montažne kutije ili podne kutije sa energetskim priključnicama.",6]
[21,"Merenje izvedene instalacije sa izradom mernog protokola",null,1]
[22,"Instalacioni materijal",null,1]
[23,"Montaža opreme i pustanje u rad",null,1]
[24,"PE 40mm","nabavka i polaganje cevi za provlačenje priključnih kablova ",40]
[]
[null,null,"UKUPAN IZNOS (DIN)"]
[]
["II","INSTALACIJA VIDEO NADZORA"]
[]
[null,"tip","opis","kol","cena","ukupno"]
[1,"KAMERA HIKVISION             DS-2CD2642 FWD-IS ","(Bullet IP kamera; Čip: 1/2.7” progressive scan CMOS 4Mpx; Rezolucija snimanja: 2688×1520@20fps; Osetljivost: 0.01 lux@F1,2, AGC on, WDR; Optika:\nvarifokal od 2,8-12mm; Interfejsi:1x RJ45, Slot za SD karticu do128GB, Audio ulaz/izlaz 1/1, Alarmni ulaz/izlaz 1/1; Protokoli: TCP/IP, Mrežni standardi: ONVIF, PSIA, CGI; IC osvetljenje: Domet IC dioda do 30m; Opšte: Napajanje 12V DC, PoE, Potrošnja 7,5W, Radna temperatura -30 ºC ~ +60 ºC, IP67)",2]
[2,"NOSAČ KAMERE ZA SPOLJNU\nMONTAŽU \nDS-1260ZJ HIKVISION   ","(Razvodna kutija za smeštanje kablova i napajanja za kamere serije DS-2CE15x2P-VFIR3, DS-2CD22x2-I i DS-\n2CD26x2F-I H)",2]
[3,"KAMERA HIKVISION             DS-2CD2142FWD-I 2.8 mm","(Dome IP kamera, Čip: 1/3” progressive scan CMOS 4Mpx, Rezolucija snimanja: 2688x1520@20fps Osetljivost: 0.01 lux@F1.2, AGC on, WDR Interfejsi:1x\nRJ45,Slot za SD karticu do 128GB Protokoli: TCP/IP, Bonjour Mrežni standardi: ONVIF, PSIA, CGI, ISAPI IC osvetljenje: Domet EXIR diode do 30m Opšte: Napajanje 12V DC, PoE, Potrošnja 5W Radna temperatura -30 ºC ~+60 ºC, IP66)",14]
[4,"NOSAC KAMERE\nDS-1280ZJ-DM18 HIKVISION   ","(Metalni nosac za kamere serije DS-2CD21xxF-I)",14]
[5,"NVR HIKVISION HKV-DS-7732NI-I4","(24-KANALNI MREŽNI SNIMAČ: Rezolucija snimanja: 8MP /6MP /5MP /4MP /3MP/1080P/UXGA/720P/VGA/ 4CIF/ DCIF/ 2CIF/CIF/QCIF, Kompresija: H.265 / H264 / H.264+ / MPEG4-Ulazno / izlazni saobraćaj: 160/160Mbps-Video/audio izlazi: HDMI/VGA: 4K (3840X2160/30Hz, 2K 2560X1440/60HZ, 1920X1080/60Hz, 1600x1200/60Hz,1280x1024/60Hz, 1280x720/60Hz, 1024X768/60Hz) 1-ch audio, RCA (2.0 Vp-p, 1 kΩ),-Dekodiranje: 2-ch @ 4K ili 8-ch @ 1080p POE interfejs: 16xRJ-45 100Mb/s, full-duplex ethernet interface, ≤200W-Dodatni ulazi: RJ45 mrežni ulaz, 1 USB 2.0 interfejs prednji,1 USB 3.0 zadnji, Alarm in/out 4/1-Hard disk prostor: 2 sata HDD do 6TB kapaciteta-Opšte: Napajanje 100-240 VAC, Potrošnja 15W bez HDD, Radna temperatura - 10 ºC ~+55 ºC)",1]
[6,"HARD DISC 4 TB","(4TB Purple, IntelliPower, SATA III, 64MB)",2]
[7,"Patch panel sa 24 RJ-45 UTP cat6","(Patch panel 19\"/1U sa 24 RJ-45 UTP cat 6 Fully Shielded)",1]
[8,"Kabal patch UTP cat6 1m","(kabal patch)",16]
[9,"Konektor RJ-45","(Konektor RJ45, Cat.5e)",16]
[10,"Kabal UTP cat.6 ","(kabal instalacioni cat.6 UTP ) (m) sporuka i montaža unutar objekta",850]
[11,"Cev instalaciona 16mm halogen free","(cevi instalacione halogen free) (m) isporuka i montaža ",600]
[12,"Instalacioni materijal",null,1]
[13,"Montaža opreme i pustanje u rad",null,1]
[]
[null,null,"UKUPAN IZNOS (DIN)"]
[]
["NAPOMENA: PNK REGALI SU SPECIFICIRANI U PROJEKTU ELEKTROENERGETSKIH INSTALACIJA."]
[]
[null,null,"REKAPITULACIJA"]
[]
[null,null,"INSTALACIJA RAČUNARSKE,TELEFONSKE I TV  INSTALACIJE"]
[null,null,"INSTALACIJA VIDEO NADZORA"]
[null,null,"UKUPNO BEZ PDV-A"]
[null,null,"PDV"]
[null,null,"UKUPNO SA PDV-OM"]